## /

## /wifi

Access Point 01
Access Point 02
Access Point 03
Access Point 04
Access Point 05
Access Point 06
Access Point 07
Access Point 08
Access Point 09
Access Point 10
100%
Access Point 11
70%
Access Point 12
10%
Access Point 13
100%
Access Point 14
66%
Access Point 15
56%
{v}
SSID
Password Show Password

### custom parameter

Label for Custom Param
{p}

#### Saving Credentials

Trying to connect ESP to network.
If it fails reconnect to AP to try again
Connected to {v}
with IP {i}
Not Connected to {v}{r}
Not Connected to apname
Authentication Failure
AP not found
Could not Connect
No AP set

#### H4 Color Header P

content

#### H4 Color Header S

content

# Heading 1

## Heading 2

### Heading 3

#### Heading 4

### WIFI HEAD (WIFI_OFF)

Chip ID
  123456
Flash Chip ID
  1234556
IDE Flash Size
  4194304 bytes
Real Flash Size
  4194304 bytes
Empty
Soft AP IP
  192.168.4.1
Soft AP MAC
  00:00:00:00:00:00
Station MAC
  00:00:00:00:00:00

### Available Pages

Page | Function
--- | ---
/ | Menu page.
/wifi | Show WiFi scan results and enter WiFi configuration.(/0wifi noscan)
/wifisave | Save WiFi configuration information and configure device. Needs variables supplied.
/close | Close the configuration server and configuration WiFi network.
/info | Information page
/close | Close the captiveportal popup,configportal will remain active
/exit | Exit Config Portal, configportal will close
/restart | Reboot the device
/erase | Erase WiFi configuration and reboot Device. Device will not reconnect to a network until new WiFi configuration data is entered.

### About

Version v1.x.x-xxxxx
Build_date
Build_file
Arduino_version

Github https://github.com/tzapu/WiFiManager
Form UPLOAD
* Upload may not function inside captive portal, Open in browser - http://192.168.4.1

Label for Custom Param
Label for Input Checkbox

Select Choice

Choice1
Choice2
Label for Input Select